**TPT03 - Vehicle Ancillary Equipment Checklist**

The following items must be checked daily under the section of Ancillary Equipment which forms part of the Drivers Daily Vehicle Check and Defect Report.

Guidance on what to check for is given below:

|  |  |  |
| --- | --- | --- |
| Vacuum Pump Oil Level |  | Check level and top up as necessary |
| Vacuum Pump Drippers |  | Check Drip Rate - 20 drips per minute |
| Vacuum Pump Exhauster |  | Check Condition/Damage/Clean as necessary |
| Vacuum Pump Mounting Bolts |  | Check Tightness |
| Vacuum Pump Engine Oil Level |  | Check level and top up as necessary |
| Vacuum Pump Engine Gear Box Oil Level |  | Check level and top up as necessary |
| Vacuum Pump Engine Fuel Level |  | Check level and top up as necessary |
| Vacuum Pump Engine Starter Rope |  | Check Condition/Damage |
| Vacuum Pump Engine Mounting Bolts |  | Check Tightness |
| Vacuum Tank Discharge Valve |  | Check Operation/Condition/Damage |
| Vacuum Tank Padlocks |  | Check Operation |
| Vacuum Tank Suction Hose(s) and Couplings |  | Check Condition/Damage |
| Vacuum Tank Suction Hose Lance and Valve  |  | Check Condition/Damage |
| Vacuum Tank Mounting Bolts  |  | Check Tightness |
| Vacuum Tank Secondary Trap |  | Check Condition/Damage/Clean as necessary |
| Vacuum Tank Sight Gauge Isolator Valves |  | Check Operation |
| Vacuum Tank Sight Gauge Volume Markers |  | Check Legible |
| Clean Water Tank |  | Check Cleanliness |
| Clean Water Tank Inlet and Outlet Valves |  | Check Operation |
| Clean Water Tank Mounting Bolts |  | Check Tightness |
| Clean Water Tank Lid and Chain |  | Check Condition/Damage |
| Clean Water Delivery Hose |  | Check Condition/Damage |
| Clean Water Pump Engine Oil Level |  | Check level and top up as necessary |
| Clean Water Pump Engine Fuel Level |  | Check level and top up as necessary |
| Clean Water Pump Engine Mounting Bolts |  | Check Tightness |
| Clean Water Pump Starter Rope |  | Check Condition/Damage |