**A1 Wokingham Car Spares**

Continuously look for pedestrians, forklifts and hazards.

Cutting Process

 **Ensure**

 **all necessary**

 **PPE**

**is worn at all times**

Begin cutting

Finish cutting

Radio completion of cutting

Let the materials cool

1. Flat surface
2. Clear of debris
3. Clear of S, T, F hazards
4. Big enough for the job

Get a crane/forklift to move materials to the bays

Yard Forman identifies need to cut

Get oxy acetylene, cutting equipment, fire extinguishers and the necessary PPE into location

Radio Banksman/team and inform them that the work is starting

Assess the best way of cutting

Use the appropriate machinery to move the material to a safe location

Locate a safe cutting area

Inspect the material