**A1 Wokingham Car Spares**

**Ensure**

**all necessary**

**PPE**

**is worn at all times**

Continuously look for pedestrians, forklifts and hazards.

Engine Shed Process

Locate vehicle with criteria suitable for export

Has the vehicle been depolluted?

Yes

No

Send to the correct depot

Depollute the vehicle

No

Yes

Use forklift to remove vehicle onto drip trays

Collect it with a forklift

Use a forklift to move to engine stock

Next one

Cut the pipes and cables with bolt cutters or a serrated knife

Unbolt the top of the engine from under bonnet

Engine tied up and engine code put on car

Use a forklift to place on the rack

Can you unbolt with airgun?

Use oxy acetylene (cutting machine)

Use a forklift to lift the car off the engine