**A1 Wokingham Car Spares**

Continuously look for pedestrians, forklifts and hazards.

Bales: all materials loading process

 **Ensure**

 **all necessary**

 **PPE**

**is worn at all times**

Easy sheet/nets

Driver tell banksman

Banksman waves the lorry into position and when it is safe the lorry will be backed up into the bay

Lorry arrives at the bottom of the hill

1. Clear room around lorry
2. Driver remains in vehicle

Banksman signals to the crane operator that it is safe to load

Crane operator will load the lorry

Crane operator to signal (beep) when completed

Crane will stop movements

Driver to exit lorry with all PPE – vehicle checks

Clear

Not clear

Go

Once all clear

Banksman to radio crane driver

Crane driver will correct