**A1 Wokingham Car Spares**

Continuously look for pedestrians, forklifts and hazards.

**Ensure**

**all necessary**

**PPE**

**is worn at all times**

Strapping vehicles - Lower Deck on 3, 5 and 8 Car Transporters

and Upper deck on 4 Car Transporter

Find a safe location to park

Put on PPE

Let someone know you have arrived and sort out necessary paperwork

Find a suitable location for loading - Ideal site should be on clear, even ground. Not near overhead cables or other possible hazards. Can you find this?

Does transporter have eyelets fitted to the body of the vehicle the car drive?

No

No

Call the office

Yes

Yes

Position lorry in a suitable position close to the vehicle

Are there any cuts or fraying to the webbing of any of the straps

Drive the vehicle into place/or attach winch to vehicle to position onto vhicle

No

Yes

Strap the vehicle into place - all four wheels where possible should be securely strapped down

Replace immediately and disposed of.

Ensure the nearside ratchet on front are pulling in opposite directions.

Double check load is secure

Check out with customer

Safely stow away ramps